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These terms apply only to the purchase of a MeasureOD® Standard software license (sometimes identified as MeasureOD® SPC) from Roth Technologies, LLC (RTA). The applicable product listing or written order identifies the license, price, supported equipment configuration, and any additional items or services included.
1. License and Purchase Scope
The one-time license price covers the MeasureOD® software license for the computer installation identified in the applicable product listing or written order. The price does not include measurement equipment, computer hardware, cables, adapters, a tower light, installation, configuration, training, or other services unless the listing or written order expressly includes them.
Any optional hardware or service, including a tower light assembly, is an additional purchase and will be charged at the price stated in the current product listing or written order.
The software license is also subject to the MeasureOD® End User License Agreement (EULA), which governs the license rights and use of the software. These purchase terms describe the commercial terms of the order. 
2. Supported Measurement Models
MeasureOD® Standard currently supports the measurement models and interfaces listed below. Measurement ranges are the manufacturers’ published ranges for the identified head types. A compatible controller, processor, interface, and configuration are required where shown.
	Manufacturer / head model
	Controller or supported interface
	Published measurement range

	Keyence LS-7010 / LS-7010M
	LS-7601
	0.04–6 mm (0.002–0.24 in)

	Keyence LS-7030 / LS-7030M
	LS-7601
	0.3–30 mm (0.01–1.18 in)

	Keyence LS-7070 / LS-7070M
	LS-7601
	0.5–65 mm (0.02–2.56 in)

	Keyence LS-9006 / LS-9006M
	LS-9501 or LS-9501P
	0.04–6 mm (0.001–0.24 in)

	Keyence LS-9030 / LS-9030M
	LS-9501 or LS-9501P
	0.3–30 mm (0.01–1.18 in)

	Keyence LS-9006D
	LS-9501 or LS-9501P; two-axis
	0.04–6 mm (0.001–0.24 in)

	Keyence LS-9030D
	LS-9501 or LS-9501P; two-axis
	0.3–30 mm (0.01–1.18 in)

	Keyence LS-9120M
	LS-9501 or LS-9501P
	0.8–120 mm (0.03–4.72 in)

	Zumbach ODAC 18XY Standard
	RS or DP interface
	0.08–15 mm (0.003–0.59 in)

	Zumbach ODAC 18XY Micro
	RS or DP interface
	0.04–15 mm (0.002–0.59 in)

	Zumbach ODAC 13TRIO
	EN-RS interface
	0.06–13 mm (0.002–0.51 in)

	Zumbach ODAC 16J
	J interface with compatible Zumbach processor/interface
	0.05–5 mm (0.002–0.20 in)

	LaserLinc TLAser122
	Applicable LaserLinc interface
	0.038–22 mm (0.0015–0.866 in)


“M” Keyence heads include a monitor camera. The LS-9006D and LS-9030D are two-axis heads. For the ODAC 18XY, both Standard and Micro versions are listed; the minimum measurement limit depends on the version. The ODAC 18XY-DP connection has been tested by RTA. Manufacturer ranges do not guarantee suitability for every material, process, or installation.
3. Buyer Equipment, Cabling and Connection Testing
Buyer is responsible for purchasing, maintaining, and providing the computer, measurement head, controller or processor, and other equipment required for the selected supported configuration. Equipment is included only when the product listing or written order expressly identifies it as included.
RTA has Keyence hardware available for connection testing. RTA does not maintain the other supported measurement systems at its offices. If Buyer requests RTA to test a connection using a non-Keyence system, Buyer must provide the applicable measurement system, controller or processor, and required interface hardware to RTA. Test scope and results depend on the equipment provided; testing is included only if expressly stated in the product listing or written order.
Buyer is responsible for providing and installing all cables, adapters, and interface hardware needed to connect the computer to the supported measurement system, including any required connection between the measurement head and its controller or processor. Requirements vary by model and interface. These items are included only if expressly listed in the product configuration or written order.
4. Computer, Windows and Network Requirements
MeasureOD® is designed to run on Windows 10 and Windows 11. Windows is not a real-time operating system, and Microsoft Windows updates may interfere with MeasureOD®’s operation or measurement timing.
Buyer is responsible for configuring the computer to prevent Windows updates from interrupting MeasureOD® or for managing updates so they are applied in a controlled manner. RTA does not configure or manage Windows updates unless expressly included in a separate written order.
An internet connection is required. Buyer is responsible for ensuring the network permits MeasureOD to communicate with RTA’s designated server at IP address 74.208.165.58 using TCP port 3306, including any necessary firewall permissions.
5. Delivery and Optional Computer Installation
After payment, RTA will coordinate software delivery or activation using the contact information supplied by Buyer. Buyer must provide accurate information needed to confirm the license and intended equipment configuration.
RTA offers to install MeasureOD® on Buyer’s computer at no charge. To use this service, Buyer must ship the computer to RTA’s offices in San Antonio, Texas, pay shipping both to RTA and for return shipping, and package the computer securely and appropriately. Buyer retains ownership of the computer and is responsible for it during shipping and the installation service. RTA is not responsible for the computer’s condition, hardware, data, or performance. RTA installs the software only and does not configure Windows update settings.
Installation, computer preparation, controller configuration, on-site work, training, custom software changes, and ongoing support are included only when expressly stated in the product listing or a separate written order. Any delivery or setup estimate will be provided separately. No specific completion date is promised unless confirmed in writing.
6. Updates and Additional Services
The one-time license price does not include updates, upgrades, maintenance, or continuing support unless the product listing or a separate written order expressly includes them. Additional services may be quoted separately.
7. Warranty and Warranty Process
RTA provides a one-year limited warranty beginning when the MeasureOD® license or software is delivered to Buyer. Buyer must notify RTA of an issue believed to prevent the system from functioning as required and provide information reasonably needed to investigate it.
RTA will investigate the reported issue and determine whether it is covered. If RTA determines that a covered issue causes the system not to function as required by the applicable product listing or written order, RTA will correct the issue. This warranty does not cover typographical errors or minor issues that do not prevent the system from functioning as required.
The warranty does not cover failures caused by Buyer-supplied hardware or Windows updates. RTA’s warranty obligation is limited to correction of an issue RTA determines is covered under this section.
8. Refunds and Cancellation
Buyer may cancel the purchase and receive a refund before delivery of the license or software. After delivery, the purchase is nonrefundable.
9. Limitation of Liability
To the fullest extent permitted by law, RTA’s total liability arising out of or relating to the applicable purchase will not exceed the purchase price paid by Buyer for that purchase. RTA will not be liable for indirect or consequential damages.
10. Governing Law
Texas law governs these terms, without regard to its conflict-of-law rules.
11. Agreement and Order Records
The product listing, these terms, and any product-specific written order describe the purchase. If a written order expressly changes a term for a particular configuration, that written change applies to that order. RTA will retain the order and checkout record.
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